Customer
Country	Name	Road	Nr	ZIP code	City

Settings	Factory settings	Installation settings
1 - PRESET
11 Unit	L
12 Decimals	0000000
13 K-Factor	0000001
14 Decimals K-Factor	0
15 Batch min	0
16 Batch max	0
2 - FLOWRATE
21 Unit	L
22 Time	/min
23 Decimals	0000000
24 K-Factor	0000001
25 Decimals K-Factor	0
26 Calculation	010
27 Cut-Off	30.0 sec.
3 - Overrun
31 Overrun	Disable
32 Time	1.0
4 - ALARM
41 No Flow	Disable
42 Time	10
5 - DISPLAY
51 Display	Increase
52 Flow Rate	Off
53 Light	100%
6 – POWER MANAGEMENT
61 LCD new	1 sec.
62 Battery Mode	Operational
7 – FLOWMETER
71 Signal	Coil-lo
8 – ANALOG
81 Output	Disable
82 Rate min.	0000000
83 Rate max.	9999999
84 Cut Off	0.0%
85 Tune min.	0208
86 Tune max.	6656
87 Filter	00 (off)
9 – RELAYS
91 Relays	1-step
92 Preclose	0
93 Width	0
94 Decimals	0
95 Amount	1000
96 Pulse	Total
A – COMMUNICATION
A1 Speed	9600
A2 Address	1
A3 Mode	BUS-RTU
B – OTHERS
B1 Model	F131-P
B2 Software version
B3 Serial Nr.
B4 Password	0000
B5 Tag-Nr.	0000000
Jumper-Settings	Int. / 3,2V

Flow Meter	Valve
Type	Serial Nr.	Type	Serial Nr.

Remarks
Engineers Name:	Date: